ARIMA HDAMA rev.I BIOS v1.23

Description:
HDMAI123.ROM = Original BIOS v1.23
HI123R55.ROM = BIOS v1.23 + Silicon Image 3114 SATA-RAID BIOS v5.5.0.0
HI123L55.ROM = BIOS v1.23 + Silicon Image 3114 SATA-Link BIOS v5.5.0.0

Instructions:
1. Upgrade to the original v1.23 BIOS first.
   This is important to upgrade the bootblock only once.
   Run HDMAI123.BAT and reboot.

2. Pick one of the modified BIOS'es:
   HI123R55.BAT => HI123R55.ROM
   HI123L55.BAT => HI123L55.ROM
