ARIMA HDAMA rev.I BIOS v1.26

Description:
HDMAI126.ROM = Original BIOS v1.26
HI126R55.ROM = BIOS v1.26 + Silicon Image 3114 SATA-RAID BIOS v5.5.0.0
HI126L55.ROM = BIOS v1.26 + Silicon Image 3114 SATA-Link BIOS v5.5.0.0

Instructions:
1. Upgrade to the original v1.26 BIOS first.
   This is important to upgrade the bootblock only once.
   Run HDMAI126.BAT and reboot.

2. Pick one of the modified BIOS'es:
   HI126R55.BAT => HI126R55.ROM
   HI126L55.BAT => HI126L55.ROM
